BACONTON COMMUNITY CHARTER SCHOOL
Pavilion Building – Construction and Finish Specifications
1. Walls and Masonry
The entire building will be constructed and finished with masonry.
Gymnasium walls will have masonry extending 10 feet above the finished floor.
The remaining gymnasium wall space above the 10-foot masonry section will receive a durable wall finish extending to the ceiling.
[bookmark: _GoBack]2. Flooring
Flooring finishes will be as follows:
Gymnasium: Finished concrete.
Both Art Rooms: Finished concrete.
Music room: Carpet tiles.
AG Mechanics: Finished concrete.
Welding Room: Finished concrete.
All Bathrooms: Epoxy flooring.
All Remaining Areas: Vinyl flooring.
3. Ceilings
Drop-down ceilings will be installed in all classrooms and offices.
The following areas will not have drop-down ceilings:
High School Art Room
AG Mechanics
Welding Room
4. Fire Protection
The building will be equipped with a complete fire sprinkler system.
All necessary equipment and components will be provided to meet applicable fire and building codes.
5. Heating, Ventilation, and Air Conditioning (HVAC)
The building will be equipped with all necessary HVAC equipment and systems.
Heating, cooling, and ventilation will be provided throughout the building to accommodate the intended use of each space.
6. Electrical
Complete electrical installation throughout the building.
All necessary lighting, outlets, switches, panels, wiring, and electrical connections will be provided.
Electrical systems will be designed to accommodate the building's intended use and equipment requirements.
7. Network and Technology
Network infrastructure and necessary data hookups will be provided throughout the building.
Classrooms, offices, and other designated areas will have the necessary network connections to support school technology needs.
8. Room Layout and Dimensions
Classroom, office, and storage closet sizes are subject to change based on the school's needs.
Room dimensions and layouts may be adjusted to maximize the available building space and best accommodate the school’s intended use.
All layout changes must remain within the overall building footprint and comply with applicable building codes and requirements.
9. General Project Requirements
The completed building will include all necessary systems, finishes, and infrastructure required for its intended use as an educational facility. Final room layouts, dimensions, and finish selections will be coordinated with Baconton Community Charter School before construction is finalized.
