


Scope for 
Fire and Rescue Tools, Equipment, and SCBA Maintenance for 
Atlanta Fire Rescue Department


This specification describes the minimum requirements for fire and rescue tools, equipment, and SCBA maintenance.

Goals and Objectives

Secure suppliers for the procurement of lumber wood and supplies, ensuring competitive pricing and availability.

Classification

The following types of fire and rescue tools, equipment, and SCBA maintenance are requested in this scope of work:

Group I       -   Powered Equipment & Accessories

Group II      -   Forcing Tools
 
Group III     -   Fire Ladders

Group IV     -   Monitors & Accessories

Group V      -   Misc. Items

Group VI     -   Self Contained Breathing Apparatus (SCBA) Air Compressor Preventive 
                         Maintenance

Specification Requirements

Bidder must provide like and similar goods or a direct substitute not listed on pricing lines at _______% discount from catalog prices.

Vendor must deliver product(s) within 45 days upon receiving a purchase order.

1. GROUP I – Powered Equipment & Accessories

1.1 RamFan EX400 Vari-Speed Dual Amp with Power shroud/Stator, Model# 
      EB80600.

1.2 RamFan OX200 16” OXH50 Powered Ventilator, Model# GG5010.

            1.3 RamFan OX350 5.5 HP Honda 18" Ventilator #GH5005 or approved equal.

            1.4 Fire Hooks Unlimited Partners K970 14” Saw.

            1.5 Super Vac PPV Electric, #718VRS.

            1.6 Super Vac 16” Ejector, #P164SE.
        
            1.7 Super Vac Door Dar for PPV, #DOORBAR or approved equal.

            1.8 Super Vac Webbing Hanging Strap for PPV,  #HR or approved equal.

            1.9 Team Saw #K970 without case.

            1.10 Piraya Diamond Rescue Saw.

                    1.10.1 Rescue Saw Blade 12”.
                    1.10.2 Rescue Saw Blade 14”.

            1.11 Team Husqvarna K970 Rescue Saw, model #K12FD or approved equal.

            1.12 Husqvarna Air Filter #510-224-41-03 or approved equal.

            1.13 Husqvarna Belt #544-9084-03 or approved equal.

            1.14 Husqvarna Spacer #506379620 or approved equal.

            1.15 Stihl Chainsaw, model #MS362 with 18” Bar.

            1.16 Stihl Chainsaw model #MS623 with 20" Bar.
                 
            1.17 Stihl Rollomatic E 18" Guide Bar, #3003 008 8917 or approved equal.

            1.18 Stihl Rollomatic E 20" Guide Bar, model #3003 000 8822 or approved equal

            1.19 Stihl Oilomatic 100’ Chain, #3623 005 1640 3/8 33RS or approved equal.

            1.20 Stihl Bar Oil, Quart Size or approved equal.

            1.21 Valvoline Motor Oil #30HD, Quart Size or approved equal.

            1.22 Stihl HP 2 Cycle Oil (6-pack) or approved equal.

            1.23 Stihl X-Line Trimmer 05, 1837 feet or approved equal.

            1.24 Exmark Hydraulic Oil Filter #109-4180 or approved equal.

            1.25 Kawasaki Oil Filter #49065-70 or approved equal.

               1.26 Napa Gold Fuel Filter #3011 or approved equal.
 
            1.27 Fire Hooks Unlimited Husky Fang 14” Diamond Saw Blade, #VCRS 14P or 
                approved equal.

            1.28 Stihl Weed Eater Head for S90 Push Down Feed or approved equal
    
            1.29 Stihl Weed Eater #FS90 with handlebars or approved equal
    
            1.30 Stihl Blower #BG55 or approved equal

            1.31 Stihl Pull Cord String or approved equal
  
            1.32 Stihl Handles or approved equal
 
            1.33 Stihl Gas Caps or approved equal

            1.34 Stihl Bar Nuts for Stihl #MS362 Chain Saw or approved equal
          
            1.35 Stihl Air Filter for Stihl #FS90 or approved equal

            1.36 Stihl Air Filters for Stihl #MS362 or approved equal
          
            1.37 Stihl Fuel Filters for Stihl #FS90 or approved equal
           
            1.38 Stihl Fuel Filters for Stihl #MS362 or approved equal
         
            1.39 Stihl Fuel Filters for Stihl #BG55 or approved equal

            1.40 Toro Air Filters for Toro 21” Kawasaki or approved equal

            1.41 Exmark Air Filters for Exmark Kawasaki or approved equal

            1.42 Warthog WH1212 Ventilation Blade

            1.43 Husqvarna Anti-Vibration Spring Model #5372103-10 or approved equal

            1.44 Husqvarna Anti-Vibration Spring Model #5372103-05 or approved equal

            1.45 Husqvarna K970 Pull Start Handle or approved equal


      2. Group II – Forcing Tools
           
           2.1 Leatherhead Tools 6 lb. Flat Axe (Yellow) 36” Handle or approved equal

           2.2 Leatherhead Tools 6 lb. Pick Head Axe (Yellow) 36” Handle or approved 
                 equal

           2.3 Leatherhead Tools 6’ NY Hook HiViz Lime Powder Coat with Chisel End & 
                 Strap or approved equal

           2.4 Leatherhead Tools 8’ NY Hook HiViz Lime Powder Coat with Chisel End &  
                 Strap or approved equal

           2.5 Leatherhead Tools 10’ NY Hook HiViz Lime Powder Coat with Chisel End & 
                 Strap or approved equal
         
           2.6 Leatherhead Tools 8’ NY Hook Black Powder Coat with Chisel End
                 or approved equal

           2.7 Leatherhead Tools 8’ NY Hook Black Powder Coat with Chisel End & Strap 
                 or approved equal
     
           2.8 Pro-Bar Halligan 30” Tool

           2.9 Nupla 10 lb. SledgeHammer with 32” Handle #26505

           2.10 Fire Hooks Unlimited 8’ Dry Wall Hook or approved equal

           2.11 Fire Hooks Unlimited 6’ Dry Wall Hook or approved equal

           2.12 Fire Hooks Unlimited CM2 Connection Mallet or approved equal

           2.13 Steck Big Easy Public Lockout Kit, #32911 or approved equal
 
           2.14 Nupla Classic Western Scoop with 48” Butt Grip Handle #72182 or approved equal

           2.15 Nupla 46.5” Black Nuplaglas Composite Pry Bar #76603 or approved equal

          2.16 Nupla 41.5” Black Nuplaglas Composite Pry Bar # 34053 or approved equal

          2.17 Worden NFPA 1901 Black Rubber Wheel Chock #HRM or approved equal

          2.18 Worden NFPA 1901 Black Rubber Wheel Chock #HRX or approved equal

          2.19 Worden HiViz Orange Urethane Wheel Chock #OUX or approved equal

          2.20 Ziamatic 6’ Pole #IBM-6 with Malleable Pike Head or approved equal

          2.21 Ziamatic 8’ Pole #IBM-8 with Malleable Pike Head or approved equal

          2.22 Ziamatic 10’ Pole #IBM-10 with Malleable Pike Head or approved equal

          2.23 Fire Hooks Unlimited 10’ Pike Pole #NY-10’ or approved equal

          2.24 Fire Hooks Unlimited 6’ Pike Poles with I-Beam fiberglass handles or 
                  approved equal
        
          2.25 Fire Hooks Unlimited 8’ Pike Poles with I-Beam fiberglass handles or 
                  approved equal

          2.26 Fire Hooks Unlimited 10’ Pike Poles with I-Beam fiberglass handles or 
                  approved equal

         2.27 Fire Hooks Unlimited 12’ Pike Poles with I-Beam fiberglass handles or 
                  approved equal

         2.28 Pike Pole Bracket (All brackets must be custom made from Aluminum for  
                  sliding out tray)

         2.29 Fire Hooks Unlimited 6’ Drywall Pulling Hooks with I-Beam fiberglass 
                  handles or approved equal

         2.30 Firehooks 30” Prybar #PB-30 or approved equal

         2.31 FlameFighter 36” Prybar #PB-36 or approved equal

         2.32 FlameFighter 60” Prybar #PB-60 or approved equal

         2.33 Southpark Raised Crowbar Holder Set #CHR55Z01C or approved equal 
    
         2.34 6 lb. Flat Head Axe with Fiberglass Handles and Bracket (All brackets must 
                 be custom made from Aluminum for sliding out tray)

         2.35 6 lb. Pick Head Axe with Fiberglass Handles and Bracket (All brackets must 
                 be custom made from Aluminum for sliding out tray)

          2.36 Bracket w/Gasket #ZSMA5201C or approved equal (All brackets 
                   must be custom made from Aluminum for sliding out tray)

          2.37 Akron 20 Ton Floor Hydraulic Jack w/Bracket or approved equal

         2.38 HK Porter Two (2) Heavy Duty Bolt Cutter w/custom fabricated mounting 
                 bracket
      
          2.39 Kline Grizzly Tool #64306 or approved equal

          2.40 Grade 100 100’ 3/8”x 10’ Tow Chain w/Clevis Strip #RC100A-799429 or 
                   approved equal  

          2.41 Grade 100 3/8”x 20’ Tow Chain #BA100S-799429 or approved equal

          2.42 3/8” Clevis Hooks
           
          2.43 3/8” Slip Hooks

          2.44 V-Bridle w/J-Hooks and T-Hooks

          2.45 8000 lb. Snatch Block w/ 4.5” Sheave

          2.46 Pike Pole Super Duty 6” Classic, #SPDH6 or approved equal

          2.47 Iron Lok, #K5003 or approved equal

          2.48 Heavy Duty Vehicle Bracket #WH01-810 (KS003 w/yellow strap) or 
                  approved equal

          2.49 Fire Hooks Unlimited A-Tool Kit #OTK-16 or approved equal
 
          2.50 Fire Hooks K-Tool or approved equal


       3. Group III – Fire Ladders

           3.1 Duo Safety 16’ Roof Ladder w/Hooks, model #875A-16

           3.2 Duo Safety 20’ Roof Ladder w/Hooks, model #875A-20

           3.3 Duo Safety 35’ 2-Section Ladder, model #1200-A-35  

           3.4 Duo Safety 28’ 2-Section Ladder, model #1200-A-28

           3.5 Duo Safety 40’ 2-Section Ladder w/ST Poles, model #1500-A

           3.6 Duo Safety 10’ Aluminum Folding Ladder, model #585-A

           3.7 Duo Safety 10’ Fresno Attic Ladder, model #701-10

           3.8 Duo Safety 12’ Fresno Attic Ladder, model #701-12

           3.9 Duo Safety 20’ 2-Section Ladder (Solid Beam), model # 900A-20

           3.10 Duo Safety 24’ 2-Section Ladder (Solid Beam), model # 900A-24

           3.11 Alco Lite 12’ Combo Ladder, model #CJL-12
 
           3.12 Duo Safety Manila Rope Coil Complete ½” x 600’, #MF-2-600

           3.13 Fire Hooks Unlimited Rex Tool or approved equal

           3.14 Duo Safety 14’ Ladder, #775A-14

           3.15 Duo Safety 28’ Ladder, #1200A-28
 
           3.16 Duo Safety 35’ Ladder, #1200A-35
       
           3.17 Duo Safety 40’ Ladder w/Stay Poles, #1500-A-40


       4. Group IV – Monitors and Accessories 

           4.1 Elkhart 2.5” FNST (Female National Standard Thread) x 2.5”, #10947004

           4.2 Elkhart 2.5” Trilock Nozzle Holder, #653

           4.3 Elkhart Brass Adapter 2.5” MNST (Male National Standard Thread) x 2.5” MNST, 
                 M327A-25
 
           4.4 Elkhart Universal Spanner Wrench, Elk-O-Lite #T464

           4.5 Elkhart Spanner Wrench Holder, #469

           4.6 Elkhart Hose and Ladder Strap, #632

           4.7 Kochee 2-Man Hose Roller, #KHR-2

           4.8 Elkhart Stream Shaper, #282-A

           4.9 Elkhart Stack Tips, #ST194

           4.10 Elkhart Key 5” HP Hose w/Storz Coupling or approved equal 

           4.11 Storz Spanner w/Mounting Bracket, #KS34

           4.12 Kocheck Adapter 5” Storz x 4” FSTN (Female Swivel Thread National Standard), 
                  #S54R54

           4.13 Kocheck Adapter 5” Storz x 4” FNPT (Female National Pipe Tapered Standard), 
                   #S37S54

           4.14 Akron Mercury Monitor Kit w/4445 Nozzle 500 GMP, #3443PK

           4.15 Kocheck Mounting Plate 4” x 5” Storz  
    
           4.16 Elkhart Adjustable Hydrant Wrench, #S454

           4.17 Elkhart Hose Clamp, #285HC

           4.18 Elkhart 5x6 Piston Intake Valve, #9786

           4.19 Elkhart 1” Booster Nozzle, #SM-3FG
 
           4.20 Elkhart Chief XD 1” Booster Nozzle

           4.21 Elkhart 1.5” Handline Nozzle, #SM–30FG
      
           4.22 Harrington Small 3-Way Ball Valve, H301 
 
           4.23 Harrington Small 2-Way Ball Valve, H201
          
           4.24 Harrington Mid-Size 2-Way Ball Valve, H202
          
           4.25 Harrington Gate Valve, HHGV
 
           4.26 Red Head 2.5” Aluminum Hydrant Gate Valve, #281A 

           4.27 Red Head Brass Expansion Ring for 1.88” Fire Hose


       5. Group V – Miscellaneous Items
         
           5.1 Akron 19000 Lumens Scene Light w/PL Base, 200Watt, 18Amp, #ELSS-XLDC-PL-  
                 PLMT

           5.2 20 lb. Dry Chemical Extinguisher Custom Fabricated Bracket
 
           5.3 Pro Line 28” Traffic Cone w/Reflective Collar Orange, or approved equal

           5.4 Short Handle Steel Pan Scoop Shovel w/”D” handle, #69014 or approved equal

           5.5 Long Handle Pointed Shovel w/Custom Fabricated Brackets, #72174 or approved  
                 equal

           5.6 Rope Bag w/200’ PMI of ½” Life Safety Rope Blue

           5.7 Rope Bag Holds 120m of 10mm Rope Red

           5.8 Fire Hooks 12 Piece Elevator Key Set, EKS-12

           5.9 Junkin Basket Stretcher, #MIL 8131-WM

           5.10 Amerex Bracket 20 #C02 Heavy Duty, #A811 or approved equal

           5.11 Bracket Bar Halligan Combo Set, #MB-PBS or approved equal

           5.12 Zico Airpak Bracket, UN-5-30-2-SF or approved equal

           5.13 South Park 3.5” Mounting Base, RMP4909AC or approved equal
 
           5.14 Access Tools Emergency Response Kit (ERK)

           5.15 Yates Large Ladderman Seat Harness #Yates- 321 or approved equal

           5.16 Yates Ladder Hook Extension Aluminum Hooks, Yates 324C or approved equal

           5.17 South Park Axe Handle Bracket w/Gasket, ZAH5101C or approved equal
 
           5.18 Worden Chock Rubber Contour Handle 8” x 7” x 10”, HRG or approved equal

           5.19 Fire Research Spectra 120V Scene Light, #Spa700-K20-0N or approved equal

           5.20 Justrite 5-Gal Red Gas Can, #7150010
    
           5.21 Justrite 5-Gal Green Gas Can, #7150400

           5.22 Justrite 2.5-Gal Yellow Gas Can, #7150200

           5.23 Radians Class 2 Safety Vest w/reflective material size: Regular w/ID Panels 4” 
                   contrasting red trim w/zip n rip, Class 2 ID panels “ATLANTA FIRE RESCUE”.

           5.24 Radians Class 2 Safety Vest w/reflective material size: Jumbo w/ID panels 4”  
                   contracting red trim w/zip n rip, Class 2 ID panels “ATLANTA FIRE RESCUE”.

           5.25 Keson Metal Professional w/Large Wheel Measuring Tape or approved equal

           5.26 Redhead Brass Hose Cutter

           5.27 Redhead Brass Expansion Rings for 1-3/4” Fire Hose 

           5.28 Redhead Brass Expansion Rings for 2 112” Fire Hose

           5.29 Redhead Brass Expansion Rings for 3” Fire Hose

           5.30 Redhead Brass 1 ¾” Aluminum Heavy Duty Expansion Ring Couplings 

           5.31 Redhead Brass 2 ½” Aluminum Heavy Duty Expansion Ring Couplings

           5.32 Redhead Brass 3” Aluminum Heavy Duty Expansion Ring Couplings 

           5.33 Redhead Brass Expansion Unit for 1 ¾”

           5.34 Redhead Brass Expansion Unit for 2 ½”
           
           5.35 Redhead Brass Expansion Unit for 3”

           5.36 Redhead Brass 2 ½” Threaded Encased Line Gauge, #155

           5.37 Crossfire Cobra Clear Safety Glasses, Model #1524

           5.38 Crossfire Cobra Smoke Safety Glasses, Model #1541

           5.39 TruFuel 50:1 - Quart Size

           5.40 TruFuel 40:1 – Quart Size

           5.41 TruFuel 4 Cycle Ethanol Free – Quart Size

                   
       6. Group VI – Self Contained Breathing Apparatus (SCBA) and Air Compressor 
           Preventive Maintenance

6.1 City of Atlanta Fire Rescue Department requests qualified, Professional Authorized 
      Firms/Distributors for the purchase, selection, care, and maintenance of Self-
      Contained Breathing Apparatus (SCBA) for Fire Rescue (FR). The successful bidder 
      will supply for the current SCBA products the corresponding parts, services, repairs, 
      and records management to ensure with the National Fire Protection Association 
      (NFPA) NFPA 1404, NFPA 1500, NFPA 1852, NFPA 1981, and NFPA 1989 as well 
      as Code of Federal Regulations (CFR) 29 CFR 1910.134 Respiratory Protection and 
      29 CFR 1910.134.

6.2 The successful bidder will provide all necessary repairs, flow tests, and establish a   
      records management system for the City of Atlanta Fire SCBA program of existing 
      equipment. Initial inventory, repair, flow test, certify, and establish a records 
      management system for the existing City of Atlanta Fire SCBA program and items 
      following: 1) 450 SCBA 2) 70 RIT Packs 3) Annual fit testing 900 employees. After 
      the inventory is established, the successful bidder will maintain all SCBA in a 
      certified state of readiness for deployment and keep a current record of all SCBA 
      owned by City of Atlanta Fire Department according to the NFPA 1500 Standard.

6.3 Preventive Maintenance: The successful bidder shall be responsible for the      
      provision of routine and emergency maintenance as well as NFPA quality testing of 
      breathing air systems. Breathing air systems shall but not limited to the compressor, 
      motor, purification devices, filters, desiccants, CO monitors, regulators, storage 
      system manifolds, valves, piping, pressure relieve devices, and fill stations. All  
      breathing air systems under this contract shall use original equipment manufacturer 
      (OEM) parts, filters, and required lubricants. All preventive maintenance shall be 
      documented on the specific manufacturer maintenance checklist or equivalent. 
      Preventative maintenance on breathing air systems shall be performed on a quarterly 
      basis. Successful bidder’s service technician shall be trained and certified in the repair 
      and maintenance of Mako, Revolve, and Bauer breathing air systems. All breathing 
      air systems maintenance, repairs, and servicing shall be recorded in the established 
      records management system.

      6.3.1 The successful bidder shall provide mobile field servicing capability for repairs  
                and inspections of SCBAs. The mobile unit must be equipped to provide  
                service in compliance with the same NFPA, OSHA, NIOSH standards as the 
                equipment in the air shop. Mobile servicing unit shall be staffed with a certified 
                Scott technician capable of making field repairs on the entire SCBA unit and 
                components. All required driver’s licensing must remain valid throughout the 
                term of the contract by the designated driver of the successful bidder.
                
                  6.3.2 The successful bidder must respond within 48 hours of the field service request.

                  6.3.3 The successful bidder will maintain all SCBA and SCBA related equipment to  
                           include but not limited to the following: 

				a) Mako Compressor System
                                          b) Revolve Air Compressor System
                                          c) Bauer Air Compressor System 
				d) All Posi-Check Equipment 
				e) All Scott Air-Pak 4500 SCBA’s  
				f) All Scott RIT Packs 
				g) All AV 3000HT Facepieces
				h) All Scott SCBA regulators 
				 i) All required parts and other required equipment not 				                stated.

         

















